Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 05 05 00 00
command: 02 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 05 05 00 00
command: 04 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 05 05 00 00
command: 05 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 05 05 00 00
command: 06 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 05 05 00 00
command: 08 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 05 05 00 00
command: 09 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 05 05 00 00
command: 0A 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 05 05 00 00
command: 0C 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 05 05 00 00
command: 0D 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 05 05 00 00
command: 0E 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 05 05 00 00
command: 10 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 05 05 00 00
command: 11 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 12 00 00 00
#
name: SLOW_UP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 13 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 14 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 15 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 05 05 00 00
command: 16 00 00 00
#
name: SLOW_DOWN
type: parsed
protocol: NECext
address: 05 05 00 00
command: 17 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 05 05 00 00
command: 18 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 05 05 00 00
command: 19 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1A 00 00 00
#
name: MEMORY
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1C 00 00 00
#
name: CLR_RST
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1D 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1E 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1F 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 20 00 00 00
#
name: BAND
type: parsed
protocol: NECext
address: 05 05 00 00
command: 23 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 05 05 00 00
command: 24 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: 05 05 00 00
command: 2B 00 00 00
#
name: FINE_UP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 2C 00 00 00
#
name: FINE_DOWN
type: parsed
protocol: NECext
address: 05 05 00 00
command: 2D 00 00 00
#
name: SHOWVIEW
type: parsed
protocol: NECext
address: 05 05 00 00
command: 30 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 05 05 00 00
command: 31 00 00 00
#
name: CLK_COUNT
type: parsed
protocol: NECext
address: 05 05 00 00
command: 33 00 00 00
#
name: PRESET
type: parsed
protocol: NECext
address: 05 05 00 00
command: 35 00 00 00
#
name: VPS
type: parsed
protocol: NECext
address: 05 05 00 00
command: 38 00 00 00
#
name: SP_LP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 3A 00 00 00
#
name: Q_PRO
type: parsed
protocol: NECext
address: 05 05 00 00
command: 3D 00 00 00
#
name: SHUTTLE_LEFT
type: parsed
protocol: NECext
address: 05 05 00 00
command: 7D 00 00 00
#
name: SHUTTLE_RIGHT
type: parsed
protocol: NECext
address: 05 05 00 00
command: 7E 00 00 00
