Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 39 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 39 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 39 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 39 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 39 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 39 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 39 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 39 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 39 00 00 00
command: 08 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 39 00 00 00
command: 0B 00 00 00
#
name: CHECK
type: parsed
protocol: NECext
address: 39 00 00 00
command: 0D 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 39 00 00 00
command: 0F 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 39 00 00 00
command: 15 00 00 00
#
name: CONTINUE
type: parsed
protocol: NECext
address: 39 00 00 00
command: 1D 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 39 00 00 00
command: 1F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 39 00 00 00
command: 20 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 39 00 00 00
command: 2C 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 39 00 00 00
command: 2E 00 00 00
#
name: POWER_ON_(CD-2)
type: parsed
protocol: NECext
address: 39 00 00 00
command: 2E 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 39 00 00 00
command: 2F 00 00 00
#
name: POWER_OFF_(CD-2)
type: parsed
protocol: NECext
address: 39 00 00 00
command: 2F 00 00 00
#
name: <<_SKIP
type: parsed
protocol: NECext
address: 39 00 00 00
command: 30 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 39 00 00 00
command: 30 00 00 00
#
name: >>_SKIP
type: parsed
protocol: NECext
address: 39 00 00 00
command: 31 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 39 00 00 00
command: 31 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 39 00 00 00
command: 32 00 00 00
#
name: <<_SEARCH
type: parsed
protocol: NECext
address: 39 00 00 00
command: 33 00 00 00
#
name: SEARCH_<<
type: parsed
protocol: NECext
address: 39 00 00 00
command: 33 00 00 00
#
name: >>_SEARCH
type: parsed
protocol: NECext
address: 39 00 00 00
command: 34 00 00 00
#
name: SEARCH_>>
type: parsed
protocol: NECext
address: 39 00 00 00
command: 34 00 00 00
#
name: SHUFFLE
type: parsed
protocol: NECext
address: 39 00 00 00
command: 35 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 39 00 00 00
command: 38 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 39 00 00 00
command: 39 00 00 00
#
name: DISC_-
type: parsed
protocol: NECext
address: 39 00 00 00
command: 3D 00 00 00
#
name: DISC_+
type: parsed
protocol: NECext
address: 39 00 00 00
command: 3E 00 00 00
#
name: DISC
type: parsed
protocol: NECext
address: 39 00 00 00
command: 4A 00 00 00
#
name: TRACK
type: parsed
protocol: NECext
address: 39 00 00 00
command: 4B 00 00 00
#
name: BLOCK
type: parsed
protocol: NECext
address: 39 00 00 00
command: 4C 00 00 00
