Filetype: IR signals file
Version: 1
#
# PENTAX Camera
# Autogenerated from ircodes/PENTAX/Camera.xml
#
name: SHUTTER
type: raw
frequency: 38000
duty_cycle: 0.33
data: 13000 3000 1000 1000 1000 1000 1000 1000 1000 1000 1000 1000 1000 1000 1000
