Filetype: IR signals file
Version: 1
#
name: ch0
type: parsed
protocol: NECext
address: 15 00 00 00
command: 00 00 00 00
#
name: ch1
type: parsed
protocol: NECext
address: 15 00 00 00
command: 01 00 00 00
#
name: ch2
type: parsed
protocol: NECext
address: 15 00 00 00
command: 02 00 00 00
#
name: ch3
type: parsed
protocol: NECext
address: 15 00 00 00
command: 03 00 00 00
#
name: ch4
type: parsed
protocol: NECext
address: 15 00 00 00
command: 04 00 00 00
#
name: ch5
type: parsed
protocol: NECext
address: 15 00 00 00
command: 05 00 00 00
#
name: ch6
type: parsed
protocol: NECext
address: 15 00 00 00
command: 06 00 00 00
#
name: ch7
type: parsed
protocol: NECext
address: 15 00 00 00
command: 07 00 00 00
#
name: ch8
type: parsed
protocol: NECext
address: 15 00 00 00
command: 08 00 00 00
#
name: ch9
type: parsed
protocol: NECext
address: 15 00 00 00
command: 09 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 15 00 00 00
command: 0D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 15 00 00 00
command: 0E 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 15 00 00 00
command: 0F 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 15 00 00 00
command: 10 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 15 00 00 00
command: 11 00 00 00
#
name: O
type: parsed
protocol: NECext
address: 15 00 00 00
command: 12 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 15 00 00 00
command: 13 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 15 00 00 00
command: 15 00 00 00
#
name: tv/vcr
type: parsed
protocol: NECext
address: 15 00 00 00
command: 16 00 00 00
#
name: prup
type: parsed
protocol: NECext
address: 15 00 00 00
command: 17 00 00 00
#
name: prdown
type: parsed
protocol: NECext
address: 15 00 00 00
command: 18 00 00 00
#
name: ad
type: parsed
protocol: NECext
address: 15 00 00 00
command: 19 00 00 00
#
name: asel
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1A 00 00 00
#
name: sp/lp
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1B 00 00 00
#
name: svc
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1C 00 00 00
#
name: A
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1D 00 00 00
#
name: gt30
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1E 00 00 00
#
name: pal/sec
type: parsed
protocol: NECext
address: 15 00 00 00
command: 1F 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 15 00 00 00
command: 21 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 15 00 00 00
command: 22 00 00 00
#
name: qs
type: parsed
protocol: NECext
address: 15 00 00 00
command: 27 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 15 00 00 00
command: 29 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 15 00 00 00
command: 31 00 00 00
#
name: indexup
type: parsed
protocol: NECext
address: 15 00 00 00
command: 33 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 15 00 00 00
command: 35 00 00 00
#
name: av
type: parsed
protocol: NECext
address: 15 00 00 00
command: 36 00 00 00
#
name: sv/v+
type: parsed
protocol: NECext
address: 15 00 00 00
command: 39 00 00 00
#
name: indexdown
type: parsed
protocol: NECext
address: 15 00 00 00
command: 3F 00 00 00
