Filetype: IR signals file
Version: 1
#
# EVO4 IP.TV SETOP BOX
# Comon used by ORANGE or O2 ISP
#
# by JEREMYNO
# 
name: POWER
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 55 AA 00 00
# 
name: ZOOM
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 4B B4 00 00
# 
name: 1
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 51 AE 00 00
# 
name: 2
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 12 ED 00 00
# 
name: 3
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 13 EC 00 00
# 
name: 4
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 4D B2 00 00
# 
name: 5
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0E F1 00 00
# 
name: 6
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0F F0 00 00
# 
name: 7
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 49 B6 00 00
# 
name: 8
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0A F5 00 00
# 
name: 9
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0B F4 00 00
# 
name: 0
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 06 F9 00 00
# 
name: TV
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 02 FD 00 00
# 
name: EPG
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 1D E2 00 00
# 
name: MENU
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 53 AC 00 00
# 
name: RECORD
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 43 BC 00 00
# 
name: PLAY
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 42 BD 00 00
# 
name: INFO
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 5F A0 00 00
# 
name: UP
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 19 E6 00 00
# 
name: DOWN
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 5A A5 00 00
# 
name: RIGHT
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 18 E7 00 00
# 
name: LEFT
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 5B A4 00 00
# 
name: OK
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 5E A1 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 07 F8 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 03 FC 00 00
# 
name: BACK
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 1C E3 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 56 A9 00 00
# 
name: CH+
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 45 BA 00 00
# 
name: CH-
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 41 BE 00 00
# 
name: REW
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 47 B8 00 00
# 
name: PLAY
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 42 BD 00 00
# 
name: STOP
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 01 FE 00 00
# 
name: FWD
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 46 B9 00 00
# 
name: PREW
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 05 FA 00 00
# 
name: TXT
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 10 EF 00 00
# 
name: AUDIO
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 11 EE 00 00
# 
name: NEXT
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 04 FB 00 00
# 
name: RED
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 4F B0 00 00
# 
name: GREEN
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 4E B1 00 00
# 
name: ORANGE
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0D F2 00 00
# 
name: BLUE
type: parsed
protocol: NECext
address: 01 FD 00 00
command: 0C F3 00 00
