Filetype: IR signals file
Version: 1
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 80 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 81 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 82 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 83 00 00 00
#
name: title-return
type: parsed
protocol: NECext
address: 00 00 00 00
command: 84 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 86 00 00 00
#
name: rev
type: parsed
protocol: NECext
address: 00 00 00 00
command: 88 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 8C 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 8D 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 8F 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 90 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 00 00 00 00
command: 91 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 00 00 00 00
command: 92 00 00 00
#
name: enter-play
type: parsed
protocol: NECext
address: 00 00 00 00
command: 93 00 00 00
#
name: repeatAB
type: parsed
protocol: NECext
address: 00 00 00 00
command: 94 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 96 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: C0 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: C1 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 00 00 00 00
command: C2 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 00 00 00 00
command: C4 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: C5 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: C6 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: C7 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: C8 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: C9 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 00 00 00 00
command: CC 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: CD 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 00 00 00 00
command: CE 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: D0 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: D1 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: D2 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: D3 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: D7 00 00 00
