Filetype: IR signals file
Version: 1
#
name: Tuner-preset+
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 00 00 00 00
#
name: Tuner-preset-
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 01 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 04 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 05 00 00 00
#
name: Tape-2
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 07 00 00 00
#
name: Tape-1
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 08 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 09 00 00 00
#
name: Phono
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 0A 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 0B 00 00 00
#
name: Deck-b-stop
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 13 00 00 00
#
name: Deck-b-play-forward
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 15 00 00 00
#
name: Deck-b-play-back
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 16 00 00 00
#
name: Deck-b-rec/pause
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 18 00 00 00
#
name: Deck-b-fastforward
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 19 00 00 00
#
name: Deck-b-rewind
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1A 00 00 00
#
name: CD-play
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1B 00 00 00
#
name: CD-stop
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1C 00 00 00
#
name: CD-next
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1D 00 00 00
#
name: CD-back
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1E 00 00 00
#
name: CD-pause
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1F 00 00 00
#
name: Tuner-class
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4A 00 00 00
#
name: Deck-a-stop
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4D 00 00 00
#
name: Deck-a-play-forward
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4E 00 00 00
#
name: Deck-a-play-back
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4F 00 00 00
#
name: Deck-a-rec/pause
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 50 00 00 00
#
name: Deck-a-fastforward
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 51 00 00 00
#
name: Deck-a-rewind
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 52 00 00 00
#
name: CD-eject
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 5C 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 5D 00 00 00
