Filetype: IR signals file
Version: 1
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: I/II
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: arrow
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 18 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: ch\*p/c
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: set
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 22 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 24 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 27 00 00 00
#
name: tv/av
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 39 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3B 00 00 00
