Filetype: IR signals file
Version: 1
# 
# Magnavox DVD NB098 remote
#
# Captured by: emptythevoid
#
name: Power
type: parsed
protocol: NECext
address: 87 22 00 00
command: 41 BE 00 00
# 
name: Display
type: parsed
protocol: NECext
address: 87 22 00 00
command: 55 AA 00 00
# 
name: Search_mode
type: parsed
protocol: NECext
address: 87 22 00 00
command: 57 A8 00 00
# 
name: Eject
type: parsed
protocol: NECext
address: 87 22 00 00
command: 44 BB 00 00
# 
name: Audio
type: parsed
protocol: NECext
address: 87 22 00 00
command: 7B 84 00 00
# 
name: Subtitle
type: parsed
protocol: NECext
address: 87 22 00 00
command: 7A 85 00 00
# 
name: Angle
type: parsed
protocol: NECext
address: 87 22 00 00
command: 79 86 00 00
# 
name: 1
type: parsed
protocol: NECext
address: 87 22 00 00
command: 45 BA 00 00
# 
name: 2
type: parsed
protocol: NECext
address: 87 22 00 00
command: 46 B9 00 00
# 
name: 3
type: parsed
protocol: NECext
address: 87 22 00 00
command: 47 B8 00 00
# 
name: 4
type: parsed
protocol: NECext
address: 87 22 00 00
command: 48 B7 00 00
# 
name: 5
type: parsed
protocol: NECext
address: 87 22 00 00
command: 49 B6 00 00
# 
name: 6
type: parsed
protocol: NECext
address: 87 22 00 00
command: 4A B5 00 00
# 
name: 7
type: parsed
protocol: NECext
address: 87 22 00 00
command: 4B B4 00 00
# 
name: 8
type: parsed
protocol: NECext
address: 87 22 00 00
command: 4C B3 00 00
# 
name: 9
type: parsed
protocol: NECext
address: 87 22 00 00
command: 4D B2 00 00
# 
name: 0
type: parsed
protocol: NECext
address: 87 22 00 00
command: 4E B1 00 00
# 
name: Clear
type: parsed
protocol: NECext
address: 87 22 00 00
command: 58 A7 00 00
# 
name: HDMI
type: parsed
protocol: NECext
address: 87 22 00 00
command: 51 AE 00 00
# 
name: Repeat
type: parsed
protocol: NECext
address: 87 22 00 00
command: 50 AF 00 00
# 
name: A_B
type: parsed
protocol: NECext
address: 87 22 00 00
command: 43 BC 00 00
# 
name: Pause
type: parsed
protocol: NECext
address: 87 22 00 00
command: 5B A4 00 00
# 
name: Skip_back
type: parsed
protocol: NECext
address: 87 22 00 00
command: 5D A2 00 00
# 
name: Skip_fwd
type: parsed
protocol: NECext
address: 87 22 00 00
command: 5F A0 00 00
# 
name: Play
type: parsed
protocol: NECext
address: 87 22 00 00
command: 5E A1 00 00
# 
name: Rev
type: parsed
protocol: NECext
address: 87 22 00 00
command: 52 AD 00 00
# 
name: Fwd
type: parsed
protocol: NECext
address: 87 22 00 00
command: 53 AC 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: 87 22 00 00
command: 60 9F 00 00
# 
name: Setup
type: parsed
protocol: NECext
address: 87 22 00 00
command: 74 8B 00 00
# 
name: Top_menu
type: parsed
protocol: NECext
address: 87 22 00 00
command: 70 8F 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 87 22 00 00
command: 71 8E 00 00
# 
name: Mode
type: parsed
protocol: NECext
address: 87 22 00 00
command: 5C A3 00 00
# 
name: Zoom
type: parsed
protocol: NECext
address: 87 22 00 00
command: 81 7E 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 87 22 00 00
command: 77 88 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 87 22 00 00
command: 75 8A 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 87 22 00 00
command: 76 89 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 87 22 00 00
command: 78 87 00 00
# 
name: Enter
type: parsed
protocol: NECext
address: 87 22 00 00
command: 72 8D 00 00
# 
name: Return
type: parsed
protocol: NECext
address: 87 22 00 00
command: 73 8C 00 00
