Filetype: IR signals file
Version: 1
#
name: MUTE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 00 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 80 00 00 00
command: 03 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 80 00 00 00
command: 04 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 80 00 00 00
command: 05 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 80 00 00 00
command: 06 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 80 00 00 00
command: 07 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 80 00 00 00
command: 08 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 80 00 00 00
command: 09 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0B 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0C 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0D 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0E 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 0F 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 10 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 80 00 00 00
command: 11 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 80 00 00 00
command: 12 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 13 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 15 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 80 00 00 00
command: 17 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 18 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 80 00 00 00
command: 19 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1A 00 00 00
#
name: X_SOURCE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1B 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1D 00 00 00
#
name: X_SNAPSHOT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 1F 00 00 00
#
name: X_SKIP_LEFT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 40 00 00 00
#
name: X_SKIP_RIGHT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 42 00 00 00
#
name: X_TIME_SHIFT
type: parsed
protocol: NECext
address: 80 00 00 00
command: 43 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 80 00 00 00
command: 44 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 80 00 00 00
command: 45 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 80 00 00 00
command: 46 00 00 00
#
name: X_REC_PLAY
type: parsed
protocol: NECext
address: 80 00 00 00
command: 47 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 80 00 00 00
command: 48 00 00 00
#
name: X_MTS
type: parsed
protocol: NECext
address: 80 00 00 00
command: 49 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 80 00 00 00
command: 4A 00 00 00
#
name: REC
type: parsed
protocol: NECext
address: 80 00 00 00
command: 4B 00 00 00
