Filetype: IR signals file
Version: 1
# 
name: Menu
type: parsed
protocol: NECext
address: EE 87 00 00
command: 02 0C 00 00
# 
name: Play_Pause
type: parsed
protocol: NECext
address: EE 87 00 00
command: 5E 0C 00 00
# 
name: Up
type: parsed
protocol: NECext
address: EE 87 00 00
command: 0B 0C 00 00
# 
name: Down
type: parsed
protocol: NECext
address: EE 87 00 00
command: 0D 0C 00 00
# 
name: Left
type: parsed
protocol: NECext
address: EE 87 00 00
command: 08 0C 00 00
# 
name: Right
type: parsed
protocol: NECext
address: EE 87 00 00
command: 07 0C 00 00
# 
name: OK
type: parsed
protocol: NECext
address: EE 87 00 00
command: 5D 0C 00 00
# 
name: Reboot
type: parsed
protocol: NECext
address: EE 87 00 00
command: 18 37 00 00
