Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 27 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 27 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 27 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 27 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 27 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 27 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 27 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 27 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 27 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 27 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 27 00 00 00
command: 0C 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 27 00 00 00
command: 20 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 27 00 00 00
command: 21 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 27 00 00 00
command: 43 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 27 00 00 00
command: 54 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 27 00 00 00
command: 55 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 27 00 00 00
command: 58 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 27 00 00 00
command: 59 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 27 00 00 00
command: 5A 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 27 00 00 00
command: 5B 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 27 00 00 00
command: 5C 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 27 00 00 00
command: 6D 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 27 00 00 00
command: 6E 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 27 00 00 00
command: 6F 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 27 00 00 00
command: 70 00 00 00
#
name: white
type: parsed
protocol: NECext
address: 27 00 00 00
command: 71 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 27 00 00 00
command: 83 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 27 00 00 00
command: 84 00 00 00
#
name: brackets
type: parsed
protocol: NECext
address: 27 00 00 00
command: AF 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 27 00 00 00
command: CB 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 27 00 00 00
command: CC 00 00 00
#
name: surf
type: parsed
protocol: NECext
address: 27 00 00 00
command: CD 00 00 00
#
name: I
type: parsed
protocol: NECext
address: 27 00 00 00
command: FD 00 00 00
