Filetype: IR signals file
Version: 1
#
name: VOL+
type: parsed
protocol: NECext
address: 47 00 00 00
command: 22 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 47 00 00 00
command: 2A 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 47 00 00 00
command: 32 00 00 00
