Filetype: IR signals file
Version: 1
# 
# Samsung BN59-01315B TV
#
name: Power
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: E6 00 00 00
# 
name: Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: Right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: Left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: Ok
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: Return
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: Home
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 79 00 00 00
# 
name: Source
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: Netflix
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: F3 00 00 00
# 
name: Prime
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: F4 00 00 00
# 
name: Vol_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: Vol_down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: Mute
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: Ch_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: Ch_down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
# 
name: Ch_list
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: 1
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 04 00 00 00
# 
name: 2
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 05 00 00 00
# 
name: 3
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 06 00 00 00
# 
name: 4
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 08 00 00 00
# 
name: 5
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 09 00 00 00
# 
name: 6
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0A 00 00 00
# 
name: 7
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0C 00 00 00
# 
name: 8
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0D 00 00 00
# 
name: 9
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0E 00 00 00
# 
name: 0
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 11 00 00 00
# 
name: Ttx_mix
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2C 00 00 00
# 
name: Pre_ch
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 13 00 00 00
# 
name: Red_a
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6C 00 00 00
# 
name: Green_b
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 14 00 00 00
# 
name: Yellow_c
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 15 00 00 00
# 
name: Blue_d
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 16 00 00 00
# 
name: Guide
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: Info
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1F 00 00 00
# 
name: Play
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 47 00 00 00
# 
name: Pause
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4A 00 00 00
# 
name: Stop
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 46 00 00 00
# 
name: Rewind
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 45 00 00 00
# 
name: Fast_fw
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 48 00 00 00
# 
name: Settings
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: Ad_subt
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 25 00 00 00
