Filetype: IR signals file
Version: 1
# 
# Viore TV LC37VF72
#
name: Power
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: Vol_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: Vol_dn
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: Vol_mute
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: Ch_next
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: Ch_prev
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
# 
name: Menu
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: Ok
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Dpad_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Dpad_down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: Dpad_left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: Dpad_right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: Back_recall
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 13 00 00 00
# 
name: Play
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Pause
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Guide
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: Info
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1F 00 00 00
# 
name: Channellist
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 26 00 00 00
# 
name: Closedcaption
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 25 00 00 00
# 
name: Favorite
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 39 00 00 00
# 
name: Input_next
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: Mts
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 00 00 00 00
# 
name: Picturemode
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 21 00 00 00
# 
name: Sleep
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 24 00 00 00
# 
name: Soundmode
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 22 00 00 00
# 
name: 1
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 04 00 00 00
# 
name: 2
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 05 00 00 00
# 
name: 3
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 06 00 00 00
# 
name: 4
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 08 00 00 00
# 
name: 5
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 09 00 00 00
# 
name: 6
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0A 00 00 00
# 
name: 7
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0C 00 00 00
# 
name: 8
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0D 00 00 00
# 
name: 9
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0E 00 00 00
# 
name: 0
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 11 00 00 00
