Filetype: IR signals file
Version: 1
# 
# Yamaha Soundbar YAS-108
# Remote Model Number VAF7640
#
name: Power
type: parsed
protocol: NEC
address: 78 00 00 00
command: CC 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 78 00 00 00
command: 1E 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 78 00 00 00
command: 1F 00 00 00
# 
name: SUB+
type: parsed
protocol: NEC
address: 78 00 00 00
command: 4C 00 00 00
# 
name: SUB-
type: parsed
protocol: NEC
address: 78 00 00 00
command: 4D 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 78 00 00 00
command: 9C 00 00 00
#
name: 3D_SURROUND
type: parsed
protocol: NEC
address: 78 00 00 00
command: C9 00 00 00
#
name: INFO
type: parsed
protocol: NEC
address: 78 00 00 00
command: 4E 00 00 00
# 
name: CLEAR_VOICE
type: parsed
protocol: NEC
address: 78 00 00 00
command: 5C 00 00 00
# 
name: SURROUND
type: parsed
protocol: NEC
address: 78 00 00 00
command: B4 00 00 00
# 
name: STEREO
type: parsed
protocol: NEC
address: 78 00 00 00
command: 50 00 00 00
#
name: HDMI
type: parsed
protocol: NEC
address: 78 00 00 00
command: 4A 00 00 00
#
name: TV
type: parsed
protocol: NEC
address: 78 00 00 00
command: DF 00 00 00
# 
name: ANALOG
type: parsed
protocol: NEC
address: 78 00 00 00
command: D1 00 00 00
#
name: BLUETOOTH
type: parsed
protocol: NEC
address: 78 00 00 00
command: 29 00 00 00
#
name: BLUETOOTH_STANDBY
type: parsed
protocol: NEC
address: 78 00 00 00
command: 34 00 00 00
#
name: DIMMER
type: parsed
protocol: NEC
address: 78 00 00 00
command: BA 00 00 00
#
name: BASE_EXTENSION
type: parsed
protocol: NEC
address: 78 00 00 00
command: 8B 00 00 00
