Filetype: IR signals file
Version: 1
# 
# Telefunken TV L55U405B4CW , JMB JT0122005B/01, Bush DLED32265HDDVDB
# Remote: RC4875
#
# On JMB/Bush non Smart TV's 
# SMART_HOME will not work.
# 
name: Power
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0C 00 00 00
# 
name: Vol_up
type: parsed
protocol: RC5
address: 01 00 00 00
command: 10 00 00 00
# 
name: Vol_dn
type: parsed
protocol: RC5
address: 01 00 00 00
command: 11 00 00 00
# 
name: Ch_next
type: parsed
protocol: RC5
address: 01 00 00 00
command: 20 00 00 00
# 
name: Ch_prev
type: parsed
protocol: RC5
address: 01 00 00 00
command: 21 00 00 00
# 
name: Up
type: parsed
protocol: RC5
address: 01 00 00 00
command: 14 00 00 00
# 
name: Down
type: parsed
protocol: RC5
address: 01 00 00 00
command: 13 00 00 00
# 
name: Left
type: parsed
protocol: RC5
address: 01 00 00 00
command: 15 00 00 00
# 
name: Right
type: parsed
protocol: RC5
address: 01 00 00 00
command: 16 00 00 00
# 
name: Ok
type: parsed
protocol: RC5
address: 01 00 00 00
command: 35 00 00 00
# 
name: Back
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0A 00 00 00
# 
name: Exit
type: parsed
protocol: RC5
address: 01 00 00 00
command: 25 00 00 00
# 
name: Smart_home
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2E 00 00 00
# 
name: Source
type: parsed
protocol: RC5
address: 01 00 00 00
command: 38 00 00 00
# 
name: Menu
type: parsed
protocol: RC5
address: 01 00 00 00
command: 30 00 00 00
# 
name: Q-menu
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2B 00 00 00
# 
name: Mute
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0D 00 00 00
# 
name: 1
type: parsed
protocol: RC5
address: 01 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: RC5
address: 01 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: RC5
address: 01 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: RC5
address: 01 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: RC5
address: 01 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: RC5
address: 01 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: RC5
address: 01 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: RC5
address: 01 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: RC5
address: 01 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: RC5
address: 01 00 00 00
command: 00 00 00 00
# 
name: Ch_list
type: parsed
protocol: RC5
address: 01 00 00 00
command: 26 00 00 00
# 
name: Prev_ch
type: parsed
protocol: RC5
address: 01 00 00 00
command: 22 00 00 00
# 
name: Info
type: parsed
protocol: RC5
address: 01 00 00 00
command: 12 00 00 00
# 
name: Usb
type: parsed
protocol: RC5
address: 01 00 00 00
command: 39 00 00 00
# 
name: P_guide
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2F 00 00 00
# 
name: 1st_ch
type: parsed
protocol: RC5
address: 01 00 00 00
command: 3B 00 00 00
# 
name: Ch_net_type
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1A 00 00 00
# 
name: Lang
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0F 00 00 00
# 
name: Subtitle
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1F 00 00 00
# 
name: Aspect
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0B 00 00 00
# 
name: Rewind
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1B 00 00 00
# 
name: Pause
type: parsed
protocol: RC5
address: 01 00 00 00
command: 31 00 00 00
# 
name: Play
type: parsed
protocol: RC5
address: 01 00 00 00
command: 19 00 00 00
# 
name: F_forward
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1C 00 00 00
# 
name: Stop
type: parsed
protocol: RC5
address: 01 00 00 00
command: 18 00 00 00
# 
name: Record
type: parsed
protocol: RC5
address: 01 00 00 00
command: 33 00 00 00
# 
name: Red
type: parsed
protocol: RC5
address: 01 00 00 00
command: 37 00 00 00
# 
name: Green
type: parsed
protocol: RC5
address: 01 00 00 00
command: 36 00 00 00
# 
name: Yellow
type: parsed
protocol: RC5
address: 01 00 00 00
command: 32 00 00 00
# 
name: Blue
type: parsed
protocol: RC5
address: 01 00 00 00
command: 34 00 00 00
